é chip revision: v0.2

I (34) boot.esp32s3: Boot SPI Speed : 80MHz

I (38) boot.esp32s3: SPI Mode       : DIO

I (43) boot.esp32s3: SPI Flash Size : 8MB

I (48) boot: Enabling RNG early entropy source...

I (53) boot: Partition Table:

I (57) boot: ## Label            Usage          Type ST Offset   Length

I (64) boot:  0 nvs              WiFi data        01 02 00009000 00006000

I (71) boot:  1 phy_init         RF data          01 01 0000f000 00001000

I (79) boot:  2 factory          factory app      00 00 00010000 00100000

I (86) boot: End of partition table

I (91) esp_image: segment 0: paddr=00010020 vaddr=3c0b0020 size=2e5ach (189868) map

I (133) esp_image: segment 1: paddr=0003e5d4 vaddr=3fc97e00 size=01a44h (  6724) load

I (135) esp_image: segment 2: paddr=00040020 vaddr=42000020 size=a0acch (658124) map

I (257) esp_image: segment 3: paddr=000e0af4 vaddr=3fc99844 size=02bbch ( 11196) load

I (260) esp_image: segment 4: paddr=000e36b8 vaddr=40374000 size=13d5ch ( 81244) load

I (289) boot: Loaded app from partition at offset 0x10000

I (289) boot: Disabling RNG early entropy source...

I (300) cpu_start: Multicore app

I (310) cpu_start: Pro cpu start user code

I (310) cpu_start: cpu freq: 160000000 Hz

I (310) cpu_start: Application information:

I (313) cpu_start: Project name:     esp32-csi-node

I (319) cpu_start: App version:      1

I (323) cpu_start: Compile time:     Mar  3 2026 04:15:10

I (329) cpu_start: ELF file SHA256:  50c89a9ed...

I (334) cpu_start: ESP-IDF:          v5.2

I (339) cpu_start: Min chip rev:     v0.0

I (344) cpu_start: Max chip rev:     v0.99 

I (349) cpu_start: Chip rev:         v0.2

I (353) heap_init: Initializing. RAM available for dynamic allocation:

I (361) heap_init: At 3FCA9468 len 000402A8 (256 KiB): RAM

I (367) heap_init: At 3FCE9710 len 00005724 (21 KiB): RAM

I (373) heap_init: At 3FCF0000 len 00008000 (32 KiB): DRAM

I (379) heap_init: At 600FE010 len 00001FD8 (7 KiB): RTCRAM

I (386) spi_flash: detected chip: gd

I (390) spi_flash: flash io: dio

I (394) sleep: Configure to isolate all GPIO pins in sleep state

I (400) sleep: Enable automatic switching of GPIO sleep configuration

I (408) main_task: Started on CPU0

I (412) main_task: Calling app_main()

I (441) nvs_config: NVS override: ssid=ruv.net

I (442) nvs_config: NVS override: password=***

I (443) nvs_config: NVS override: target_ip=192.168.1.20

I (448) nvs_config: NVS override: wasm_verify=0

I (452) main: ESP32-S3 CSI Node (ADR-018) â?? Node ID: 1

I (460) pp: pp rom version: e7ae62f

I (462) net80211: net80211 rom version: e7ae62f

I (469) wifi:wifi driver task: 3fcb3784, prio:23, stack:6656, core=0

I (489) wifi:wifi firmware version: cc1dd81

I (489) wifi:wifi certification version: v7.0

I (489) wifi:config NVS flash: enabled

I (490) wifi:config nano formating: disabled

I (494) wifi:Init data frame dynamic rx buffer num: 32

I (499) wifi:Init static rx mgmt buffer num: 5

I (503) wifi:Init management short buffer num: 32

I (507) wifi:Init dynamic tx buffer num: 32

I (511) wifi:Init static tx FG buffer num: 2

I (515) wifi:Init static rx buffer size: 2212

I (519) wifi:Init static rx buffer num: 16

I (523) wifi:Init dynamic rx buffer num: 32

I (527) wifi_init: rx ba win: 16

I (531) wifi_init: tcpip mbox: 32

I (535) wifi_init: udp mbox: 32

I (538) wifi_init: tcp mbox: 6

I (542) wifi_init: tcp tx win: 5760

I (546) wifi_init: tcp rx win: 5760

I (550) wifi_init: tcp mss: 1440

I (554) wifi_init: WiFi IRAM OP enabled

I (559) wifi_init: WiFi RX IRAM OP enabled

I (566) phy_init: phy_version 620,ec7ec30,Sep  5 2023,13:49:13

I (612) wifi:mode : sta (3c:0f:02:ec:c2:28)

I (612) wifi:enable tsf

I (614) main: WiFi STA initialized, connecting to SSID: ruv.net

I (623) wifi:new:<5,0>, old:<1,0>, ap:<255,255>, sta:<5,0>, prof:1

I (625) wifi:state: init -> auth (b0)

I (656) wifi:state: auth -> assoc (0)

I (749) wifi:state: assoc -> run (10)

