# Functional Specification
## WiFi-DensePose System

### Document Information
- **Version**: 1.0
- **Date**: 2025-01-07
- **Project**: InvisPose - WiFi-Based Dense Human Pose Estimation
- **Status**: Draft

---

## 1. Introduction

### 1.1 Purpose
This document defines the functional requirements and behaviors of the WiFi-DensePose system, specifying what the system must do to meet user needs across healthcare, retail, and security domains.

### 1.2 Scope
The functional specification covers all user-facing features, system behaviors, data processing workflows, and integration capabilities required for the WiFi-based human pose estimation platform.

### 1.3 Functional Overview
The system transforms WiFi Channel State Information (CSI) into real-time human pose estimates through neural network processing, providing privacy-preserving human sensing capabilities with 87.2% accuracy.

---

## 2. Core Functional Requirements

### 2.1 CSI Data Collection and Processing

#### 2.1.1 WiFi Signal Acquisition
**Function**: Extract Channel State Information from compatible WiFi routers
- **Input**: Raw WiFi signals from 3×3 MIMO antenna arrays
- **Processing**: Real-time CSI extraction with amplitude and phase data
- **Output**: Structured CSI data streams with temporal coherence
- **Frequency**: Continuous operation at 10-30 Hz sampling rate

**Acceptance Criteria**:
- Successfully extract CSI from Atheros-based routers
- Maintain data integrity across extended operation periods
- Handle network interruptions with automatic reconnection
- Support multiple router types with unified data format

#### 2.1.2 Signal Preprocessing
**Function**: Clean and normalize raw CSI data for neural network input
- **Phase Unwrapping**: Correct phase discontinuities and wrapping artifacts
- **Temporal Filtering**: Apply moving average and linear detrending
- **Background Subtraction**: Remove static environmental components
- **Noise Reduction**: Filter systematic noise and interference

**Processing Pipeline**:
```
Raw CSI → Phase Unwrapping → Temporal Filtering → 
Background Subtraction → Noise Reduction → Normalized CSI
```

**Acceptance Criteria**:
- Achieve signal-to-noise ratio improvement of 10dB minimum
- Maintain temporal coherence across processing stages
- Adapt to environmental changes automatically
- Process data streams without introducing latency >10ms

#### 2.1.3 Environmental Calibration
**Function**: Establish baseline measurements for background subtraction
- **Baseline Capture**: Record empty environment CSI patterns
- **Adaptive Calibration**: Update baselines for environmental changes
- **Multi-Environment**: Support different room configurations
- **Drift Compensation**: Correct for systematic signal drift

**Calibration Process**:
1. Capture 60-second baseline with no human presence
2. Establish statistical models for background variation
3. Monitor for environmental changes requiring recalibration
4. Update baselines automatically or on user request

### 2.2 Neural Network Inference

#### 2.2.1 Modality Translation Network
**Function**: Convert 1D CSI signals to 2D spatial representations
- **Dual-Branch Processing**: Separate amplitude and phase encoders
- **Feature Fusion**: Combine modality-specific features
- **Spatial Upsampling**: Generate 720×1280 spatial representations
- **Temporal Consistency**: Maintain coherence across frames

**Network Architecture**:
```
CSI Input (3×3×N) → Amplitude Branch → Feature Fusion → 
Phase Branch → Upsampling → Spatial Features (720×1280×3)
```

**Performance Requirements**:
- Processing latency <50ms on GPU hardware
- Maintain temporal consistency across frame sequences
- Support batch processing for efficiency
- Graceful degradation on CPU-only systems

#### 2.2.2 DensePose Estimation
**Function**: Extract dense human pose from spatial features
- **Body Part Detection**: Identify 24 anatomical regions
- **UV Coordinate Mapping**: Generate dense correspondence maps
- **Keypoint Extraction**: Detect 17 major body keypoints
- **Confidence Scoring**: Provide detection confidence metrics

**Output Format**:
- Dense pose masks for 24 body parts
- UV coordinates for surface mapping
- 2D keypoint coordinates with confidence scores
- Bounding boxes for detected persons

#### 2.2.3 Multi-Person Tracking
**Function**: Track multiple individuals across frame sequences
- **Person Detection**: Identify up to 5 individuals simultaneously
- **ID Assignment**: Maintain consistent person identifiers
- **Occlusion Handling**: Track through temporary occlusions
- **Trajectory Smoothing**: Apply temporal filtering for stability

**Tracking Features**:
- Kalman filtering for position prediction
- Hungarian algorithm for ID assignment
- Confidence-based track management
- Automatic track initialization and termination

### 2.3 Real-Time Processing Pipeline

#### 2.3.1 Data Flow Management
**Function**: Orchestrate end-to-end processing pipeline
- **Buffer Management**: Handle continuous data streams
- **Queue Processing**: Manage processing queues efficiently
- **Resource Allocation**: Optimize CPU/GPU utilization
- **Error Recovery**: Handle processing failures gracefully

**Pipeline Stages**:
1. CSI Data Ingestion
2. Preprocessing and Normalization
3. Neural Network Inference
4. Post-processing and Tracking
5. Output Generation and Distribution

#### 2.3.2 Performance Optimization
**Function**: Maintain real-time performance under varying loads
- **Adaptive Processing**: Scale processing based on available resources
- **Frame Dropping**: Skip frames under high load conditions
- **Batch Optimization**: Group operations for efficiency
- **Memory Management**: Prevent memory leaks and optimize usage

**Optimization Strategies**:
- Dynamic batch size adjustment
- GPU memory pooling
- Asynchronous processing pipelines
- Intelligent frame scheduling

---

## 3. User Stories and Use Cases

### 3.1 Healthcare Domain User Stories

#### 3.1.1 Elderly Care Monitoring
**As a** healthcare provider
**I want** to monitor elderly patients for fall events and activity patterns
**So that** I can provide immediate assistance and track health trends

**Acceptance Criteria**:
- System detects falls with 95% accuracy within 2 seconds
- Activity patterns are tracked and reported daily
- Alerts are sent immediately upon fall detection
- Privacy is maintained with no video recording

**User Journey**:
1. Caregiver configures fall detection sensitivity
2. System continuously monitors patient movement
3. Fall event triggers immediate alert to caregiver
4. System provides activity summary for health assessment

// TEST: Verify fall detection accuracy meets 95% threshold
// TEST: Confirm activity tracking provides meaningful health insights
// TEST: Validate alert delivery within 2-second requirement

#### 3.1.2 Rehabilitation Progress Tracking
**As a** physical therapist
**I want** to track patient movement and exercise compliance
**So that** I can adjust treatment plans based on objective data

**Acceptance Criteria**:
- Exercise movements are accurately classified
- Progress metrics are calculated and visualized
- Compliance rates are tracked over time
- Integration with electronic health records

**User Journey**:
1. Therapist sets up exercise monitoring protocol
2. Patient performs prescribed exercises
3. System tracks movement quality and completion
4. Progress reports are generated for treatment planning

// TEST: Verify exercise classification accuracy for rehabilitation movements
// TEST: Confirm progress metrics calculation and visualization
// TEST: Validate EHR integration functionality

### 3.2 Retail Domain User Stories

#### 3.2.1 Store Layout Optimization
**As a** retail manager
**I want** to understand customer traffic patterns and zone popularity
**So that** I can optimize store layout and product placement

**Acceptance Criteria**:
- Customer paths are tracked anonymously
- Zone dwell times are measured accurately
- Heatmaps show traffic density patterns
- A/B testing capabilities for layout changes

**User Journey**:
1. Manager configures store zones and tracking areas
2. System monitors customer movement throughout day
3. Analytics dashboard shows traffic patterns and insights
4. Manager uses data to optimize store layout

// TEST: Verify anonymous customer tracking maintains privacy
// TEST: Confirm zone analytics provide actionable insights
// TEST: Validate A/B testing framework for layout optimization

#### 3.2.2 Queue Management
**As a** store operations manager
**I want** to monitor checkout queue lengths and wait times
**So that** I can optimize staffing and reduce customer wait times

**Acceptance Criteria**:
- Queue lengths are detected in real-time
- Wait times are calculated automatically
- Staff alerts when queues exceed thresholds
- Historical data for staffing optimization

**User Journey**:
1. Manager sets queue length and wait time thresholds
2. System monitors checkout areas continuously
3. Alerts are sent when thresholds are exceeded
4. Historical data guides staffing decisions

// TEST: Verify queue detection accuracy in various store layouts
// TEST: Confirm wait time calculations are precise
// TEST: Validate alert system for queue management

### 3.3 Security Domain User Stories

#### 3.3.1 Perimeter Security Monitoring
**As a** security officer
**I want** to monitor restricted areas for unauthorized access
**So that** I can respond quickly to security breaches

**Acceptance Criteria**:
- Intrusion detection works through walls and obstacles
- Real-time alerts with location information
- Integration with existing security systems
- Audit trail for all security events

**User Journey**:
1. Security officer configures restricted zones
2. System monitors areas 24/7 without line-of-sight
3. Intrusion triggers immediate alert with location
4. Officer responds based on alert information

// TEST: Verify through-wall detection capability
// TEST: Confirm real-time alert delivery with accurate location
// TEST: Validate integration with security management systems

#### 3.3.2 Building Occupancy Monitoring
**As a** facility manager
**I want** to track building occupancy for safety and compliance
**So that** I can ensure emergency evacuation procedures and capacity limits

**Acceptance Criteria**:
- Accurate person counting in all monitored areas
- Real-time occupancy dashboard
- Emergency evacuation support
- Compliance reporting for safety regulations

**User Journey**:
1. Manager configures occupancy limits for each area
2. System tracks person count continuously
3. Dashboard shows real-time occupancy status
4. Emergency mode provides evacuation support

// TEST: Verify person counting accuracy across different environments
// TEST: Confirm occupancy dashboard provides real-time updates
// TEST: Validate emergency evacuation support functionality

---

## 4. Real-Time Streaming Requirements

### 4.1 Performance Requirements

#### 4.1.1 Latency Requirements
**End-to-End Latency**: <100ms from CSI data to pose output
- CSI Processing: <20ms
- Neural Network Inference: <50ms
- Post-processing and Tracking: <20ms
- API Response Generation: <10ms

**Streaming Latency**: <50ms for WebSocket delivery
- Internal Processing: <30ms
- Network Transmission: <20ms

// TEST: Verify end-to-end latency meets <100ms requirement
// TEST: Confirm WebSocket streaming latency <50ms
// TEST: Validate latency consistency under varying loads

#### 4.1.2 Throughput Requirements
**Processing Throughput**: 10-30 FPS depending on hardware
- Minimum: 10 FPS on CPU-only systems
- Optimal: 20 FPS on GPU-accelerated systems
- Maximum: 30 FPS on high-end hardware

**Concurrent Streaming**: Support 100+ simultaneous clients
- WebSocket connections: 100 concurrent
- REST API clients: 1000 concurrent
- Streaming bandwidth: 10 Mbps per client

// TEST: Verify processing throughput meets FPS requirements
// TEST: Confirm system supports 100+ concurrent streaming clients
// TEST: Validate bandwidth utilization stays within limits

### 4.2 Data Streaming Architecture

#### 4.2.1 Multi-Protocol Support
**WebSocket Streaming**: Primary real-time protocol
- Binary and JSON message formats
- Compression for bandwidth optimization
- Automatic reconnection handling
- Client-side buffering for smooth playback

**Server-Sent Events (SSE)**: Alternative streaming protocol
- HTTP-based streaming for firewall compatibility
- Automatic retry and reconnection
- Event-based message delivery
- Browser-native support

**MQTT Streaming**: IoT ecosystem integration
- QoS levels for reliability guarantees
- Topic-based message routing
- Retained messages for state persistence
- Scalable pub/sub architecture

// TEST: Verify WebSocket streaming handles reconnections gracefully
// TEST: Confirm SSE provides reliable alternative streaming
// TEST: Validate MQTT integration with IoT ecosystems

#### 4.2.2 Adaptive Streaming
**Quality Adaptation**: Automatic quality adjustment based on network conditions
- Bandwidth detection and monitoring
- Dynamic frame rate adjustment
- Compression level optimization
- Graceful degradation strategies

**Client Capability Detection**: Optimize streaming for client capabilities
- Device performance assessment
- Network bandwidth measurement
- Display resolution adaptation
- Battery optimization for mobile clients

// TEST: Verify adaptive streaming adjusts to network conditions
// TEST: Confirm client capability detection works accurately
// TEST: Validate quality adaptation maintains user experience

### 4.3 Restream Integration Specifications

#### 4.3.1 Platform Support
**Supported Platforms**: Multi-platform simultaneous streaming
- YouTube Live: RTMP streaming with custom overlays
- Twitch: Real-time pose visualization streams
- Facebook Live: Social media integration
- Custom RTMP: Enterprise and private platforms

**Stream Configuration**: Flexible streaming parameters
- Resolution: 720p, 1080p, 4K support
- Frame Rate: 15, 30, 60 FPS options
- Bitrate: Adaptive 1-10 Mbps
- Codec: H.264, H.265 support

// TEST: Verify simultaneous streaming to multiple platforms
// TEST: Confirm stream quality meets platform requirements
// TEST: Validate custom RTMP endpoint functionality

#### 4.3.2 Visualization Pipeline
**Pose Overlay Generation**: Real-time visualization creation
- Skeleton rendering with customizable styles
- Confidence indicators and person IDs
- Background options (transparent, solid, custom)
- Multi-person color coding

**Stream Composition**: Video stream assembly
- Pose overlay compositing
- Background image/video integration
- Text overlay for metadata
- Logo and branding integration

**Performance Optimization**: Efficient video processing
- GPU-accelerated rendering
- Parallel processing pipelines
- Memory-efficient operations
- Real-time encoding optimization

// TEST: Verify pose overlay generation meets quality standards
// TEST: Confirm stream composition handles multiple elements
// TEST: Validate performance optimization maintains real-time processing

#### 4.3.3 Stream Management
**Connection Management**: Robust streaming infrastructure
- Automatic reconnection on failures
- Stream health monitoring
- Bandwidth adaptation
- Error recovery procedures

**Analytics and Monitoring**: Stream performance tracking
- Viewer count monitoring
- Stream quality metrics
- Bandwidth utilization tracking
- Error rate monitoring

**Configuration Management**: Dynamic stream control
- Real-time parameter adjustment
- Stream start/stop control
- Platform-specific optimizations
- Scheduled streaming support

// TEST: Verify stream management handles connection failures
// TEST: Confirm analytics provide meaningful insights
// TEST: Validate configuration changes apply without interruption

---

## 5. Domain-Specific Functional Requirements

### 3.1 Healthcare Monitoring

#### 3.1.1 Fall Detection
**Function**: Detect and alert on fall events for elderly care
- **Pattern Recognition**: Identify rapid position changes
- **Threshold Configuration**: Adjustable sensitivity settings
- **Alert Generation**: Immediate notification on fall detection
- **False Positive Reduction**: Filter normal activities

**Detection Algorithm**:
```
Pose Trajectory Analysis → Velocity Calculation → 
Position Change Detection → Confidence Assessment → Alert Decision
```

**Alert Criteria**:
- Vertical position change >1.5m in <2 seconds
- Horizontal impact detection
- Sustained ground-level position >10 seconds
- Configurable sensitivity thresholds

#### 3.1.2 Activity Monitoring
**Function**: Track patient mobility and activity patterns
- **Activity Classification**: Identify sitting, standing, walking, lying
- **Mobility Metrics**: Calculate movement frequency and duration
- **Inactivity Detection**: Alert on prolonged inactivity periods
- **Daily Reports**: Generate activity summaries

**Monitored Activities**:
- Walking patterns and gait analysis
- Sitting/standing transitions
- Sleep position monitoring
- Exercise and rehabilitation activities

#### 3.1.3 Privacy-Preserving Analytics
**Function**: Generate health insights while protecting patient privacy
- **Anonymous Data**: No personally identifiable information
- **Aggregated Metrics**: Statistical summaries only
- **Secure Storage**: Encrypted local data storage
- **Audit Trails**: Comprehensive access logging

### 3.2 Retail Analytics

#### 3.2.1 Customer Traffic Analysis
**Function**: Monitor customer movement and behavior patterns
- **Traffic Counting**: Real-time customer count tracking
- **Zone Analytics**: Movement between store zones
- **Dwell Time**: Time spent in specific areas
- **Path Analysis**: Customer journey mapping

**Analytics Outputs**:
- Hourly/daily traffic reports
- Zone popularity heatmaps
- Average dwell time by area
- Peak traffic period identification

#### 3.2.2 Occupancy Management
**Function**: Monitor store capacity and density
- **Real-Time Counts**: Current occupancy levels
- **Capacity Alerts**: Notifications at threshold levels
- **Queue Detection**: Identify waiting areas and lines
- **Social Distancing**: Monitor spacing compliance

**Capacity Features**:
- Configurable occupancy limits
- Real-time dashboard displays
- Automated alert systems
- Historical occupancy trends

#### 3.2.3 Layout Optimization
**Function**: Provide insights for store layout improvements
- **Traffic Flow**: Identify bottlenecks and dead zones
- **Product Interaction**: Monitor engagement with displays
- **Conversion Analysis**: Path-to-purchase tracking
- **A/B Testing**: Compare layout configurations

### 3.3 Security Applications

#### 3.3.1 Intrusion Detection
**Function**: Monitor restricted areas for unauthorized access
- **Perimeter Monitoring**: Detect boundary crossings
- **Through-Wall Detection**: Monitor without line-of-sight
- **Behavioral Analysis**: Identify suspicious movement patterns
- **Real-Time Alerts**: Immediate security notifications

**Detection Capabilities**:
- Motion detection in restricted zones
- Loitering detection with configurable timeouts
- Multiple person alerts
- Integration with security systems

#### 3.3.2 Access Control Integration
**Function**: Enhance physical security systems
- **Zone-Based Monitoring**: Different security levels by area
- **Time-Based Rules**: Schedule-dependent monitoring
- **Credential Correlation**: Link with access card systems
- **Audit Logging**: Comprehensive security event logs

#### 3.3.3 Emergency Response
**Function**: Support emergency evacuation and response
- **Occupancy Tracking**: Real-time person counts by zone
- **Evacuation Monitoring**: Track movement during emergencies
- **First Responder Support**: Provide occupancy information
- **Emergency Alerts**: Automated emergency notifications

---

## 4. API and Integration Functions

### 4.1 REST API Endpoints

#### 4.1.1 Pose Data Access
**Endpoints**:
- `GET /pose/latest` - Current pose data
- `GET /pose/history` - Historical pose data
- `GET /pose/stream` - Real-time pose stream
- `POST /pose/query` - Custom pose queries

**Response Format**:
```json
{
  "timestamp": "2025-01-07T04:46:32Z",
  "persons": [
    {
      "id": 1,
      "confidence": 0.87,
      "keypoints": [...],
      "dense_pose": {...},
      "bounding_box": {...}
    }
  ],
  "metadata": {
    "processing_time": 45,
    "frame_id": 12345
  }
}
```

#### 4.1.2 System Control
**Endpoints**:
- `POST /system/start` - Start pose estimation
- `POST /system/stop` - Stop pose estimation
- `GET /system/status` - System health status
- `POST /system/calibrate` - Trigger calibration

#### 4.1.3 Configuration Management
**Endpoints**:
- `GET /config` - Current configuration
- `PUT /config` - Update configuration
- `GET /config/templates` - Available templates
- `POST /config/validate` - Validate configuration

### 4.2 WebSocket Streaming

#### 4.2.1 Real-Time Data Streams
**Function**: Provide low-latency pose data streaming
- **Connection Management**: Handle multiple concurrent clients
- **Message Broadcasting**: Efficient data distribution
- **Automatic Reconnection**: Client reconnection handling
- **Rate Limiting**: Prevent client overload

**Stream Types**:
- Pose data streams
- System status updates
- Alert notifications
- Performance metrics

#### 4.2.2 Client Management
**Function**: Manage WebSocket client lifecycle
- **Authentication**: Secure client connections
- **Subscription Management**: Topic-based subscriptions
- **Connection Monitoring**: Health check and cleanup
- **Error Handling**: Graceful error recovery

### 4.3 External Integration

#### 4.3.1 MQTT Publishing
**Function**: Integrate with IoT ecosystems
- **Topic Structure**: Hierarchical topic organization
- **Message Formats**: JSON and binary message support
- **QoS Levels**: Configurable quality of service
- **Retained Messages**: State persistence

**MQTT Topics**:
- `wifi-densepose/pose/person/{id}` - Individual pose data
- `wifi-densepose/alerts/{type}` - Alert notifications
- `wifi-densepose/status` - System status
- `wifi-densepose/analytics/{domain}` - Domain analytics

#### 4.3.2 Webhook Integration
**Function**: Send real-time notifications to external services
- **Event Triggers**: Configurable event conditions
- **Retry Logic**: Automatic retry on failures
- **Authentication**: Support for various auth methods
- **Payload Customization**: Flexible message formats

**Webhook Events**:
- Person detection/departure
- Fall detection alerts
- System status changes
- Threshold violations

#### 4.3.3 Restream Integration
**Function**: Live streaming to multiple platforms
- **Multi-Platform**: Simultaneous streaming to multiple services
- **Video Encoding**: Real-time video generation
- **Stream Management**: Automatic reconnection and quality adaptation
- **Overlay Generation**: Pose visualization overlays

---

## 5. User Interface Functions

### 5.1 Web Dashboard

#### 5.1.1 Real-Time Visualization
**Function**: Display live pose estimation results
- **Pose Rendering**: Real-time skeleton visualization
- **Multi-Person Display**: Color-coded person tracking
- **Confidence Indicators**: Visual confidence representation
- **Background Options**: Configurable visualization backgrounds

**Visualization Features**:
- Stick figure pose representation
- Dense pose heat maps
- Keypoint confidence visualization
- Trajectory tracking displays

#### 5.1.2 System Monitoring
**Function**: Monitor system health and performance
- **Performance Metrics**: Real-time performance indicators
- **Resource Usage**: CPU, GPU, memory utilization
- **Network Status**: CSI data stream health
- **Error Reporting**: System error and warning displays

#### 5.1.3 Configuration Interface
**Function**: System configuration and control
- **Parameter Adjustment**: Real-time parameter tuning
- **Template Selection**: Domain-specific configuration templates
- **Calibration Control**: Manual calibration triggers
- **Alert Configuration**: Threshold and notification settings

### 5.2 Mobile Interface

#### 5.2.1 Responsive Design
**Function**: Mobile-optimized interface for monitoring
- **Touch Interface**: Mobile-friendly controls
- **Responsive Layout**: Adaptive screen sizing
- **Offline Capability**: Basic functionality without connectivity
- **Push Notifications**: Mobile alert delivery

#### 5.2.2 Quick Actions
**Function**: Essential controls for mobile users
- **System Start/Stop**: Basic system control
- **Alert Acknowledgment**: Quick alert responses
- **Status Overview**: System health summary
- **Emergency Controls**: Rapid emergency response

---

## 6. Data Management Functions

### 6.1 Data Storage

#### 6.1.1 Pose Data Storage
**Function**: Store pose estimation results for analysis
- **Time-Series Storage**: Efficient temporal data storage
- **Compression**: Data compression for storage efficiency
- **Indexing**: Fast query performance
- **Retention Policies**: Configurable data retention

**Storage Schema**:
```
pose_data:
  - timestamp (primary key)
  - person_id
  - pose_keypoints
  - confidence_scores
  - metadata
```

#### 6.1.2 Configuration Storage
**Function**: Persist system configuration and settings
- **Version Control**: Configuration change tracking
- **Backup/Restore**: Configuration backup capabilities
- **Template Management**: Pre-configured templates
- **Validation**: Configuration integrity checking

#### 6.1.3 Analytics Storage
**Function**: Store aggregated analytics and reports
- **Domain-Specific**: Separate storage for different domains
- **Aggregation**: Pre-computed analytics for performance
- **Export Capabilities**: Data export in multiple formats
- **Privacy Compliance**: Anonymized data storage

### 6.2 Data Processing

#### 6.2.1 Batch Analytics
**Function**: Process historical data for insights
- **Trend Analysis**: Long-term pattern identification
- **Statistical Analysis**: Comprehensive statistical metrics
- **Report Generation**: Automated report creation
- **Data Mining**: Advanced pattern discovery

#### 6.2.2 Real-Time Analytics
**Function**: Generate live insights from streaming data
- **Stream Processing**: Real-time data aggregation
- **Threshold Monitoring**: Live threshold violation detection
- **Anomaly Detection**: Real-time anomaly identification
- **Alert Generation**: Immediate alert processing

---

## 7. Quality Assurance Functions

### 7.1 Testing and Validation

#### 7.1.1 Automated Testing
**Function**: Comprehensive automated test coverage
- **Unit Testing**: Component-level test coverage
- **Integration Testing**: End-to-end pipeline testing
- **Performance Testing**: Load and stress testing
- **Regression Testing**: Continuous validation

#### 7.1.2 Hardware Simulation
**Function**: Test without physical hardware
- **CSI Simulation**: Synthetic CSI data generation
- **Scenario Testing**: Predefined test scenarios
- **Environment Simulation**: Various deployment conditions
- **Validation Testing**: Algorithm validation

### 7.2 Monitoring and Diagnostics

#### 7.2.1 System Health Monitoring
**Function**: Continuous system health assessment
- **Performance Monitoring**: Real-time performance tracking
- **Resource Monitoring**: Hardware resource utilization
- **Error Detection**: Automatic error identification
- **Predictive Maintenance**: Proactive issue identification

#### 7.2.2 Diagnostic Tools
**Function**: Troubleshooting and problem resolution
- **Log Analysis**: Comprehensive log analysis tools
- **Performance Profiling**: Detailed performance analysis
- **Network Diagnostics**: CSI data stream analysis
- **Debug Interfaces**: Developer debugging tools

---

## 8. Acceptance Criteria

### 8.1 Functional Acceptance
- **Pose Detection**: Successfully detect human poses with 87.2% AP@50
- **Multi-Person**: Track up to 5 individuals simultaneously
- **Real-Time**: Maintain <100ms end-to-end latency
- **Domain Functions**: All domain-specific features operational

### 8.2 Integration Acceptance
- **API Endpoints**: All specified endpoints functional
- **WebSocket Streaming**: Real-time data streaming operational
- **External Integration**: MQTT, webhooks, and Restream functional
- **Dashboard**: Web interface fully operational

### 8.3 Performance Acceptance
- **Throughput**: Achieve 10-30 FPS processing rates
- **Reliability**: 99.5% uptime over testing period
- **Scalability**: Support 100+ concurrent API clients
- **Resource Usage**: Operate within specified hardware limits

// TEST: Validate CSI data extraction from all supported router types
// TEST: Verify neural network inference accuracy meets AP@50 targets
// TEST: Confirm multi-person tracking maintains ID consistency
// TEST: Validate real-time performance under various load conditions
// TEST: Test all API endpoints for correct functionality
// TEST: Verify WebSocket streaming handles multiple concurrent clients
// TEST: Validate domain-specific functions for healthcare, retail, security
// TEST: Confirm external integrations work with MQTT, webhooks, Restream
// TEST: Test web dashboard functionality across different browsers
// TEST: Validate data storage and retrieval operations
// TEST: Verify system monitoring and diagnostic capabilities
// TEST: Confirm automated testing framework covers all components