# RuView · Cinematic

ADR-097 · pseudo-CSI visualization layer
Subject● Tracked
Pose walking
Heart rate— bpm
Breathing— bpm
Mesh nodes 4 · multistatic
Coherence— %
Tomography idle
Bbox vol— m³
Render— fps

## Helpers · ADR-097

GridHelper PolarGridHelper BoxHelper AxesHelper Per-node BoxHelpers Sonar pings Tomography sweep

## Per-node CSI · synthetic

N1·BL
—
N2·BR
—
N3·FL
—
N4·FR
—
CSI amplitude derived from distance-to-keypoint + Doppler + thermal noise. Drives bone glow, ping coherence, tomography trigger threshold.
RuView · Seldon Vault
multistatic wifi pose · ADR-097
ADR-097 · three.js helpers · cinematic